>> MIB - Management Information Base
>> Table: udp - (.1.3.6.1.2.1.7)
udp
OID | Name | Type | Access
.1 | InDatagrams | Counter32 | R
.2 | NoPorts | Counter32 | R
.3 | InErrors | Counter32 | R
.4 | OutDatagrams | Counter32 | R
InDatagrams
The total number of UDP datagrams delivered to UDP users.
NoPorts
The total number of received UDP datagrams for which there was no application at the destination port.
InErrors
The number of received UDP datagrams that could not be delivered for reasons other than the lack of an application at the destination port.
OutDatagrams
The total number of UDP datagrams sent from this entity.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH