>> MIB - Management Information Base
>> Table: wlcPresenceServerTable - (.1.3.6.1.4.1.272.4.61.1.40.1)
Description: Contains all collection servers defined by the user.
wlcPresenceServerTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | ProfIndex | INTEGER | RW
.3 | Address | DisplayString | RW
.4 | Secret | DisplayString | RW
.5 | Validator | DisplayString | RW
.6 | RowStatus | ENUM | D
Index
Unique index of the server.
ProfIndex
Index of the 'wlcPresenceProfile' entry used for this server.
Address
Collection server address. The server address starts with 'http' or 'https', providing this last option security mechanisms, followed by an IP address or a domain name with an optional port number separated by a colon. An aditional resource address can be appended at the end of this field. Length: 0 to 255
Secret
Secret string used by the collection server for accepting incoming messages. Length: 0 to 255
Validator
Organization-specific validator string. The one provided by the collection server must match this one. Length: 0 to 255
RowStatus
The row-status of a server entry. Enumerations: active (1) notInService (2) notReady (3) createAndGo (4) createAndWait (5) destroy (6)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH