>> MIB - Management Information Base
>> Table: localTcpLimitTable - (.1.3.6.1.4.1.272.4.5.14.3.1)
Description: Table to be used to limit access to local TCP services.
localTcpLimitTable
OID | Name | Type | Access
.1 | AdminState | ENUM | D
.2 | Service | ENUM | RW
.3 | MaxSessions | INTEGER | RW
.4 | CurSessions | Counter | R
.5 | State | ENUM | R
AdminState
The administrative state of this limit entry. Enumerations: active (1) inactive (2) delete (3)
Service
The corresponding TCP service. Enumerations: telnet (1) trace (2) snmp (3) capi (4) tapi (5) rfc1086 (6) http (7) https (8) ssh (9)
MaxSessions
Maximum number of allowed sessions for this TCP service. Range: 0 to 65536
CurSessions
The current number of sessions for this TCP service.
State
The current state for this TCP service. Enumerations: below (1) exceeded (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH