>> MIB - Management Information Base
>> Table: tr069ParameterTable - (.1.3.6.1.4.1.272.4.22.6.9.1.1)
Description: Table to save values and attributes for TR069 parameter values are only saved if no native MIB is available and necessary. E.g. Alias values (if the values is not valid and notification is default this entry could be removed.
tr069ParameterTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | ObjIdx | INTEGER | RW
.3 | ID | INTEGER | RW
.4 | Value | DisplayString | RW
.5 | ValueState | ENUM | RW
.6 | Notification | ENUM | RW
.7 | State | ENUM | RW
Index
Table index.
ObjIdx
parent object index
ID
Representation of the parameter (type) name as number
Value
parameter value Length: 0 to 50
ValueState
Value is valid or not valid Enumerations: valid (1) not-valid (2)
Notification
Representation of notificationt setting for this parameter (set from ACS) no - not notification passive - changed vales will be send with next INFROM active - a value change will trigger an INFORM default - defautl notification for this parameter Enumerations: no (0) passive (1) active (2) default (3)
State
Entry is valid or delete it Enumerations: valid (1) delete (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH