>> MIB - Management Information Base
>> Table: wlcLocalServicesProfileTable - (.1.3.6.1.4.1.272.4.61.1.15.1)
Description: This table contains configuration profiles for local services (e.g. httpd, sshd) on the WTP.
wlcLocalServicesProfileTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | AdminStatus | ENUM | D
.3 | Name | DisplayString | RW
.4 | Port | INTEGER | RW
.5 | PortRange | INTEGER | RW
.6 | Protocol | ENUM | RW
Index
Unique local services profile index
AdminStatus
The administrative status of this entry. The entry can be enabled(1), disabled(2) or set to delete(32) and is therefore deleted. Default is enabled(1). Enumerations: enabled (1) disabled (2) delete (32)
Name
The name of the ServicesProfile entry. Length: 0 to 63
Port
The port number. Range: -1 to 65535
PortRange
The port range. Range: 1 to 65536
Protocol
The protocol type of this entry. Enumerations: icmp (1) igmp (2) ip (4) tcp (6) udp (17) udptcp (253) any (254) dont-verify (256)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH