>> MIB - Management Information Base
>> Table: ipsecTrafficSelectorTable - (.1.3.6.1.4.1.272.4.26.35.1)
Description: This object contains an IPSec security association.
ipsecTrafficSelectorTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | PeerIndex | INTEGER | R
.3 | BundleIndex | INTEGER | R
.4 | IpVersion | ENUM | R
.5 | Proto | ENUM | R
.6 | LocalAddress | IpAddress | R
.7 | LocalRange | IpAddress | R
.8 | LocalIp6Address | InetAddressIPv6 | R
.9 | LocalIp6Range | InetAddressIPv6 | R
.10 | LocalMaskLen | INTEGER | R
.11 | RemoteAddress | IpAddress | R
.12 | RemoteRange | IpAddress | R
.13 | RemoteIp6Address | InetAddressIPv6 | R
.14 | RemoteIp6Range | InetAddressIPv6 | R
.15 | RemoteMaskLen | INTEGER | R
.16 | LocalPort | INTEGER | R
.17 | LocalPortRange | INTEGER | R
.18 | RemotePort | INTEGER | R
.19 | RemotePortRange | INTEGER | R
.20 | ChildXrt | INTEGER | R
Index
A unique index for this entry.
PeerIndex
The index of the peer for which this traffic selector was created.
BundleIndex
The index of the bundle for which this traffic selector was created.
IpVersion
Used IP version of this traffic selector: ipv4 -- IPv4 ipv6 -- IPv6
Proto
The protocol of the traffic selector.
LocalAddress
The local IPv4 address (host or network or range start address) of the traffic selector.
LocalRange
The local IPv4 address range end address of the traffic selector.
LocalIp6Address
The local IPv6 address (host or network or range start address) of the traffic selectors.
LocalIp6Range
The local IPv6 address range end address of the traffic selector.
LocalMaskLen
The local IPv4 or IPv6 network masklen of the traffic selector (in combination with ipsecTrafficSelectorAddress).
RemoteAddress
The remote IPv4 address (host or network or range start address) of the traffic selector.
RemoteRange
The remote IPv4 address range end address of the traffic selector.
RemoteIp6Address
The remote IPv6 address (host or network or range start address) of the traffic selectors.
RemoteIp6Range
The remote IPv6 address range end address of the traffic selector.
RemoteMaskLen
The remote IPv4 or IPv6 network masklen of the traffic selector (in combination with ipsecTrafficSelectorAddress).
LocalPort
The local port of the traffic selector.
LocalPortRange
The local port range end port of the traffic selector.
RemotePort
The remote port of the traffic selector.
RemotePortRange
The remote port range end port of the traffic selector.
ChildXrt
Row number of the associated ipExtRtTable entry.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH