>> MIB - Management Information Base
>> Table: timeServerTable - (.1.3.6.1.4.1.272.4.1.54.1)
Description: This object contains a time server entry.
timeServerTable
OID | Name | Type | Access
.1 | Priority | INTEGER | RW
.2 | Protocol | ENUM | D
.3 | Address | DisplayString | RW
Priority
The priority of the time server. The time servers are queried in the order of ascending priority value, i.e. 0 first, 1 second ... . Range: 0 to 128
Protocol
The protocol used for the time server. Enumerations: delete (1) time-udp (2) time-tcp (3) sntp (4) disabled (5)
Address
The IP Address or DNS name of the time server. If a DNS name is specified here, it is resolved on demand. Length: 0 to 255

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH