>> MIB - Management Information Base
>> Table: xotStatTable - (.1.3.6.1.4.1.272.4.32.2.1)
Description: The xotStatTable contains statistical connection- specific information. Only the system can add or delete entries to this table. Creating entries: Entries are created by the system each time a new XOT interface is created in the xotIfTable. Deleting entries: Entries are removed by the system when the corresponding XOT interface is removed.
xotStatTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | OutgoingCalls | Counter | R
.3 | IncomingCalls | Counter | R
.4 | PktsSent | Counter | R
.5 | PktsRecvd | Counter | R
.6 | OutgoingFails | Counter | R
.7 | IncomingFails | Counter | R
IfIndex
Correlating XOT interface index.
OutgoingCalls
The number of outgoing calls on this interface since its last change to the 'up' state.
IncomingCalls
The number of incoming calls on this interface since its last change to the 'up' state.
PktsSent
The number of transmitted packets on this interface since its last change to the 'up' state.
PktsRecvd
The number of received packets on this interface since its last change to the 'up' state.
OutgoingFails
The number of outgoing call failures on this interface since its last change to the 'up' state.
IncomingFails
The number of incoming call failures on this interface since its last change to the 'up' state.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH