>> MIB - Management Information Base
>> Table: lispRemSiteTable - (.1.3.6.1.4.1.272.4.23.9.2.1)
Description: List of remote LISP-sites (see section 4.1 of RFC-6833). For each pair of remote and local site of same LISP-instance, a corresponding entry is stored in ipExtRtTable.
lispRemSiteTable
OID | Name | Type | Access
.1 | InstId | INTEGER | RW
.2 | Addr | IpAddress | RW
.3 | Len | INTEGER | RW
.4 | Aligned | IpAddress | R
.5 | AdminStatus | ENUM | D
InstId
Refers to lispInstId-field of related lispInst-entry. Range: -1 to 16777215
Addr
Together with lispRemSiteLen, specifies EID-prefix of this remote LISP-site. Cached EID-prefixes (received via Map-Reply) may (but should not) be completely different ones. In such cases, LISP-routing considers only such IP-frames that match with both kinds of prefixes, administratively configured one and dynamically received ones.
Len
See description of lispRemSiteAddr. Converted/stored as ipExtRtDstMask in related ipExtRt-entries. Range: 0 to 32
Aligned
Prefix-length-aligned read-only-version of lispRemSiteAddr. Stored as ipExtRtDstAddr in related ipExtRt-entries
AdminStatus
Administrative status of remote LISP-site. Set to delete for killing entry. Enumerations: active (1) inactive (2) delete (3)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH