>> MIB - Management Information Base
>> Table: ipHostAccessStat - (.1.3.6.1.4.1.272.4.5.62.3)
ipHostAccessStat
OID | Name | Type | Access
.1 | LoginCnt | INTEGER | RW
.2 | LoginTime | Date | R
.3 | CurClientsCnt | INTEGER | R
.4 | MaxClientsCnt | INTEGER | RW
.5 | MaxClientsTime | Date | R
.6 | RedirectCnt | INTEGER | RW
.7 | RedirectTime | Date | R
.8 | MaxClientsLimit | INTEGER | R
LoginCnt
The number of client-login-attempts since system-start. Any write-access causes reset to 0.
LoginTime
Last time when ipHostAccessStatLoginCnt was set. Range: 0 to -1
CurClientsCnt
The current number of authenticated or pending clients. Further login-attempts are rejected if this value already reached ipHostAccessStatMaxClientsLimit.
MaxClientsCnt
The maximum observed value of ipHostAccessStatCurClientsCnt since system-start. Any write-access causes initialisation to current value of ipHostAccessStatCurClientsCnt.
MaxClientsTime
Last time when ipHostAccessStatMaxClientsCnt was set. Range: 0 to -1
RedirectCnt
The number of redirects to local HTTP-server since system-start. Any write-access causes reset to 0.
RedirectTime
Last time when ipHostAccessStatRedirectCnt was set. Range: 0 to -1
MaxClientsLimit
Maximum allowed value for ipHostAccessStatCurClientsCnt. Any login-attempts beyond this limit are rejected.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH