>> MIB - Management Information Base
>> Table: tr069FileTransferTable - (.1.3.6.1.4.1.272.4.22.6.5.1.1)
Description: An entry containing information about one pending up- or download.
tr069FileTransferTable
OID | Name | Type | Access
.2 | Type | ENUM | RW
.3 | Direction | ENUM | RW
.4 | URL | DisplayString | RW
.5 | Username | DisplayString | RW
.6 | Password | DisplayString | RW
.7 | CommandKey | DisplayString | RW
.8 | StartTime | INTEGER | RW
.9 | CompleteTime | INTEGER | RW
.10 | FaultCode | INTEGER | RW
Type
Type of file to up- or download. Enumerations: firmware (1) configuration (2) log (3)
Direction
Direction of the file transfer. Enumerations: download (1) upload (2)
URL
URL to contact for the up- / download. Length: 0 to 256
Username
Username to be used to authenticate with the file server. Length: 0 to 256
Password
Password to be used to authenticate with the file server. Length: 0 to 256
CommandKey
Opaque parameter to be sent along with a TransferComplete RPC. Length: 0 to 32
StartTime
Time the transfer starts.
CompleteTime
Time the transfer completed.
FaultCode
Fault code related to this file transfer.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH