>> MIB - Management Information Base
>> Table: trcBufStat - (.1.3.6.1.4.1.272.4.1.65.3)
trcBufStat
OID | Name | Type | Access
.1 | NUnused | Unsigned32 | R
.2 | NOpen | Unsigned32 | R
.3 | NFull | Unsigned32 | R
NUnused
Number of trace buffers currently available to store data.
NOpen
Number of trace buffers currently available for appending data.
NFull
Number of trace buffers currently available for reading data only (i.e. in state 'full').

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH