>> MIB - Management Information Base
>> Table: mcastFwdTable - (.1.3.6.1.4.1.272.4.5.53.1)
Description: An entry in the Multicast Forwarding Table.
mcastFwdTable
OID | Name | Type | Access
.1 | Address | IpAddress | RW
.2 | SrcIfIndex | INTEGER | RW
.3 | DestIfIndex | INTEGER | RW
.4 | Status | ENUM | D
Address
The multicast forwarding group address which will be forwarded. The group address 224.0.0.0 may be used as a wildcard matching all addresses.
SrcIfIndex
The source interface of incoming multicast packets.
DestIfIndex
The destination interface where to forward multicast packets.
Status
The status of this entry. Enumerations: active (1) inactive (2) delete (3)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH