>> MIB - Management Information Base
>> Table: guiAdmin - (.1.3.6.1.4.1.272.4.69.1.1)
guiAdmin
OID | Name | Type | Access
.1 | VideoHelpUrl | DisplayString | RW
.2 | Autosave | ENUM | RW
.3 | Settings | BITS | RW
VideoHelpUrl
Specifies a URL where video help support is available. Length: 0 to 255
Autosave
This value determines if GUI auto save is enabled (true) or disabled (false). Enumerations: true (1) false (2)
Settings
Gui Settings: showManufacturerNames: This value determines if the Ethernet vendor codes and well-known MAC addresses are shown Enumerations: showManufacturerNames (0)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH