>> MIB - Management Information Base
>> Table: biboAdmLicInfoTable - (.1.3.6.1.4.1.272.4.1.32.1)
Description: This table contains an entry for each feature, that can be activated by a license. The licenses have to be entered in the biboAdmLicenseTable. This tabl indicates the current state of the different licenses.
biboAdmLicInfoTable
OID | Name | Type | Access
.1 | Type | ENUM | R
.2 | Status | ENUM | R
.3 | Id | DisplayString | R
.4 | Slot | INTEGER | R
.5 | MaxLic | Counter32 | R
.6 | InUse | Counter32 | R
.7 | HwSerial | DisplayString | R
.8 | Unit | INTEGER | R
.9 | Limit | Counter32 | R
.10 | Free | Counter32 | R
Type
The licenseable feature. Enumerations: ip (1) capi (2) bridge (3) x25 (4) ipx (5) stac (6) frame-relay (7) tapi (8) ospf (9) extended-lan (10) tunneling (11) taf (12) extended-wan (13) leased-line (14) lcr (15) app-power-phone (17) app-operator-desk (18) app-voice-mail-server (19) app-accounting-tool (20) app-intelligent-voice (21) app-6 (22) e25 (29) ipsec (33) ipseccb-ipxfer (34) bgp (35) uefs (36) siplan (37) siptrunk (38) pim (39) call-by-call (40) fax (41) sipout (42) brrp (43) wlan-controller (44) terminal-option (45) data-encr-accel (46) voice-mail-system (47) pptp (48) ethernet (128) bri (129) g703 (130) pri (131) modem (132) g7032pri (133) slots (134) e3 (135) serial (136) shdsl (137) vdsl (138)
Status
The current state of the license. Enumerations: builtin (1) valid-license (2) invalid-license (3) no-license (4) erase-internal (5)
Id
The complete serial id string of the special license. Length: 0 to 255
Slot
In case of a hardware license corresponding to a dedicated module serial number, it is the slot number of the module. Range: 0 to 255
MaxLic
The max number of allowed chunks.
InUse
The current number of chunks in use.
HwSerial
The complete serial id string of the special license. Length: 0 to 255
Unit
In case of a hardware license corresponding to a dedicated module serial number, it is the unit number of the module. Range: 0 to 255
Limit
The maximum number of licenseable chunks.
Free
The number of free default licences.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH