>> MIB - Management Information Base
>> Table: ip6DhcpStats - (.1.3.6.1.4.1.272.4.5.100.4.2)
ip6DhcpStats
OID | Name | Type | Access
.1 | InSolicit | Counter32 | R
.2 | InRequest | Counter32 | R
.3 | InConfirm | Counter32 | R
.4 | InRenew | Counter32 | R
.5 | InRebind | Counter32 | R
.6 | InRelease | Counter32 | R
.7 | InDecline | Counter32 | R
.8 | InInfoReq | Counter32 | R
.9 | InRelayForw | Counter32 | R
.10 | InRelayRepl | Counter32 | R
.11 | InUnknown | Counter32 | R
.12 | OutAdvertise | Counter32 | R
.13 | OutReply | Counter32 | R
.14 | OutReconf | Counter32 | R
.15 | OutRelayForw | Counter32 | R
.16 | OutRelayRepl | Counter32 | R
InSolicit
Number of received Solicit messages (see 5.3 of RFC-3315).
InRequest
Number of received Request messages (see 5.3 of RFC-3315).
InConfirm
Number of received Confirm messages (see 5.3 of RFC-3315).
InRenew
Number of received Renew messages (see 5.3 of RFC-3315).
InRebind
Number of received Rebind messages (see 5.3 of RFC-3315).
InRelease
Number of received Release messages (see 5.3 of RFC-3315).
InDecline
Number of received Decline messages (see 5.3 of RFC-3315).
InInfoReq
Number of received Information-request messages (see 5.3 of RFC-3315).
InRelayForw
Number of received Relay-forward messages (see 5.3 of RFC-3315).
InRelayRepl
Number of received Relay-reply messages (see 5.3 of RFC-3315).
InUnknown
Number of received messages of unknown type (see 5.3 of RFC-3315).
OutAdvertise
Number of sent Advertise messages (see 5.3 of RFC-3315).
OutReply
Number of sent Reply messages (see 5.3 of RFC-3315).
OutReconf
Number of sent Reconfigure messages (see 5.3 of RFC-3315).
OutRelayForw
Number of sent Relay-forward messages (see 5.3 of RFC-3315).
OutRelayRepl
Number of sent Relay-reply messages (see 5.3 of RFC-3315).

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH