>> MIB - Management Information Base
>> Table: ipWalledGardenAddressTable - (.1.3.6.1.4.1.272.4.5.62.6.1)
Description: An entry representing an IP address for which host access authentication is enabled.
ipWalledGardenAddressTable
OID | Name | Type | Access
.1 | DomainOperIndex | INTEGER | R
.2 | Network | IpAddress | R
DomainOperIndex
The parent index in ipWalledGardenDomainOperTable with same value for ipWalledGardenDomainOperIndex.
Network
This object specifies together with ipWalledGardenAddressNetmask the network where hosts can communicate without authorization.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH