>> MIB - Management Information Base
>> Table: wlcKnownAPTable - (.1.3.6.1.4.1.272.4.61.1.30.1)
Description: This table contains a list of known AP's and how they should be handled.
wlcKnownAPTable
OID | Name | Type | Access
.1 | BSSID | MacAddress | RC
.2 | LastSeen | Date | R
.3 | Type | ENUM | D
.4 | Description | DisplayString | RC
BSSID
The BSSID of the rouge AP. Length: 6 to 6
LastSeen
The timestamp, when this known AP was last seen. Range: 0 to -1
Type
This attribute contains the type of the well known AP. If it is set to 'neighborhood' but the found AP is also a rogue the rogue message will still be displayed. If it is set to 'rogue' no message for either neighborhood or rogue appears. Set this value to 'delete' to remove this entry. Enumerations: neighborhood (2) rogue (3) delete (15)
Description
A user defined description for this known AP. Length: 0 to 255

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH