>> MIB - Management Information Base
>> Table: mobilePLMNTable - (.1.3.6.1.4.1.272.4.41.4.1.27.1)
Description: A single mobilePLMNTable entry.
mobilePLMNTable
OID | Name | Type | Access
.1 | Code | INTEGER | R
.2 | Name | DisplayString | R
Code
The PLMN (Public Land Mobile Network) code of the network operator. This code is merged from the MCC (Mobile Country Code) and MNC (Mobile Network Code) of the network operator.
Name
The name of the network operator. Length: 0 to 20

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH