>> MIB - Management Information Base
>> Table: mon4geSysStatTable - (.1.3.6.1.4.1.272.4.41.5.1.2.1)
Description: A single mon4geSysStatTable entry.
mon4geSysStatTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | OperStatus | ENUM | R
.3 | SysDescr | DisplayString | R
.4 | SysName | DisplayString | R
.5 | SysUpTime | TimeTicksFIX | R
.6 | Manufacturer | DisplayString | R
.7 | Model | DisplayString | R
.8 | Release | DisplayString | R
.9 | IMEI | DisplayString | R
.10 | Temperature | INTEGER | R
.11 | SIM | DisplayString | R
.12 | ICCId | DisplayString | R
.13 | RegState | ENUM | R
.14 | Roaming | DisplayString | R
.15 | PLMN | INTEGER | R
.16 | Provider | DisplayString | R
.17 | ConnState | DisplayString | R
.18 | ConnTime | INTEGER | R
.19 | RAT | DisplayString | R
.20 | Band | DisplayString | R
.21 | CSQ | INTEGER | R
.22 | Bandwidth | DisplayString | R
.23 | LAC | INTEGER | R
.24 | CellId | INTEGER | R
.25 | LTECellId | INTEGER | R
.26 | IpAddress | DisplayString | R
.27 | DNS1 | DisplayString | R
.28 | DNS2 | DisplayString | R
.29 | RxBytes | Counter32 | R
.30 | RxPackets | Counter32 | R
.31 | TxBytes | Counter32 | R
.32 | TxPackets | Counter32 | R
.33 | RxBpsLast1m | Counter32 | R
.34 | TxBpsLast1m | Counter32 | R
.35 | RxBpsLast5m | Counter32 | R
.36 | TxBpsLast5m | Counter32 | R
.37 | TxStartsFailure | Counter32 | R
.38 | TxSkbAllocsFailure | Counter32 | R
.39 | TxCompletionsWithErr | Counter32 | R
.40 | TxCompletionsOutSeq | Counter32 | R
.41 | RxCompletionsWrongB | Counter32 | R
.42 | RxMissed | Counter32 | R
.43 | RxErrsInDriver | Counter32 | R
Index
Index reference to mon4geSysConfigEntry.
OperStatus
Operational state of the device Enumerations: up (1) down (2)
SysDescr
Attached system description Length: 0 to 255
SysName
Attached system name. Length: 0 to 255
SysUpTime
Attached system uptime.
Manufacturer
Cellular module manufacturer. Length: 0 to 255
Model
Cellular module model. Length: 0 to 255
Release
Cellular module firmware release. Length: 0 to 255
IMEI
Cellular module IMEI. Length: 0 to 255
Temperature
Cellular module temperature.
SIM
Cellular mobile SIM status. Length: 0 to 255
ICCId
Cellular active SIM ICC. Length: 0 to 255
RegState
Cellular mobile registration state. Enumerations: searching (0) home-network (1) attaching (2) denied (3) unknown (4) roaming (5)
Roaming
Current Roaming status. Length: 0 to 255
PLMN
Public land mobile network used (PLMN).
Provider
Network name of public land mobile. Length: 0 to 255
ConnState
Call state. Length: 0 to 255
ConnTime
Current connection time.
RAT
Cellular mobile current radio access tecnology used. Length: 0 to 255
Band
Cellular mobile current active band. Length: 0 to 255
CSQ
Cellular mobile signal versus noise ratio (SINR).
Bandwidth
Cellular negotiated bandwidth in Kbps. Length: 0 to 255
LAC
Cellular mobile cell location area code.
CellId
Cellular mobile used cell id.
LTECellId
Cellular mobile used LTE cell id.
IpAddress
Cellular mobile assigned IP Address. Length: 0 to 255
DNS1
Cellular mobile assigned primary DNS Server. Length: 0 to 255
DNS2
Cellular mobile assigned secondary DNS Server. Length: 0 to 255
RxBytes
Number of data bytes received by the radio interface
RxPackets
Number of data packtes received by the radio interface
TxBytes
Number of data bytes sent by the radio interface.
TxPackets
Number of data packtes sent by the radio interface.
RxBpsLast1m
Rx throughput measured in the last minute in bps.
TxBpsLast1m
Rx throughput measured in the last minute in bps.
RxBpsLast5m
Rx throughput measured in the last five minutes in bps.
TxBpsLast5m
Tx throughput measured in the last five minutes in bps.
TxStartsFailure
Transmission packets start failure.
TxSkbAllocsFailure
Transmission packets skb allocs failure.
TxCompletionsWithErr
Transmission packets completed with errors.
TxCompletionsOutSeq
Transmission packets completed out of sequence.
RxCompletionsWrongB
Received packets completed wrong b.
RxMissed
Received packets missed.
RxErrsInDriver
Received packets for errors in driver.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH