>> MIB - Management Information Base
>> Table: hwAccelChanStatTable - (.1.3.6.1.4.1.272.4.63.1.3.1)
Description: This object contains the statistic info for a HW accelerator channel.
hwAccelChanStatTable
OID | Name | Type | Access
.1 | Slot | INTEGER | R
.2 | Unit | INTEGER | R
.3 | Chan | INTEGER | R
.4 | CurrSessions | Counter32 | R
.5 | MaxSessions | Counter32 | R
.9 | Errors | Counter32 | R
.10 | LastError | TimeTicks | R
.11 | Resets | Counter32 | R
.12 | LastReset | TimeTicks | R
.13 | DoneOverflows | Counter32 | R
.14 | LastDoneOverflow | TimeTicks | R
Slot
The slot number of this HW accelerator entry.
Unit
The unit number of this HW accelerator entry.
Chan
The channel number of this HW accelerator entry.
CurrSessions
The current number of sessions handled by this HW accelerator channel.
MaxSessions
The maximum number of sessions handled by this HW accelerator channel.
Errors
The number of errors for this HW accelerator channel.
LastError
The time passed since the last error for this HW accelerator channel.
Resets
The number of HW accelerator channel resets.
LastReset
The time passed since the last HW accelerator channel reset.
DoneOverflows
The number of done overflow conditions for this HW accelerator channel.
LastDoneOverflow
The time passed since the last done overflow condition for this HW accelerator channel.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH