>> MIB - Management Information Base
>> Table: ip6SifAliasTable - (.1.3.6.1.4.1.272.4.5.100.1.8.1)
Description: Contains a IPv6 'Stateful Inspection Firewall' (SIF) policy.
ip6SifAliasTable
OID | Name | Type | Access
.1 | Order | INTEGER | RW
.2 | Source | INTEGER | RW
.3 | Destination | INTEGER | RW
.4 | Service | INTEGER | RW
.5 | Action | ENUM | D
.6 | Status | ENUM | RW
.7 | Priority | ENUM | RW
.8 | ClassId | INTEGER | RW
.9 | Dscp | INTEGER | RW
Order
The configured order (implict priority) for this 'Stateful Inspection Firewall' (SIF) rule.
Source
The source index associated with this rule.
Destination
The destination index associated with this rule.
Service
The protocol/service associated with this rule.
Action
The policy associated with this rule. Enumerations: access (1) deny (2) reject (3) delete (255)
Status
Defines the administrative status of this rule. Enumerations: enabled (1) disabled (2)
Priority
Defines the QoS priority associated with this rule. Enumerations: default (1) low-latency (2) high (3) medium (4) low (5)
ClassId
Internal ID for SIF policy to QoS policy mapping Range: 0 to 255
Dscp
DSCP value to be set for signalling Range: 0 to 63

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH