>> MIB - Management Information Base
>> Table: dot1dTp - (.1.3.6.1.4.1.272.4.8.4)
dot1dTp
OID | Name | Type | Access
.1 | LearnedEntryDiscards | Counter | R
.2 | AgingTime | INTEGER | RW
LearnedEntryDiscards
The total number of Forwarding Database entries, which have been or would have been learnt, but have been discarded due to a lack of space to store them in the Forwarding Database. If this counter is increasing, it indicates that the Forwarding Database is regularly becoming full (a condition which has unpleasant performance effects on the subnetwork). If this counter has a significant value but is not presently increasing, it indicates that the problem has been occurring but is not persistent.
AgingTime
The timeout period in seconds for aging out dynamically learned forwarding information. Range: 10 to 1000000

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH