>> MIB - Management Information Base
>> Table: mpsUserUserTable - (.1.3.6.1.4.1.272.4.53.6.18.1)
Description: This table contains additional information for the user.
mpsUserUserTable
OID | Name | Type | Access
.1 | Index | UserIndex | RW
.2 | Pin | DisplayString | RW
.3 | AdminStatus | ENUM | D
.4 | Facilities | BITS | RW
Index
A unique value for each user, referencing to mpsUserIndex in mpsUserTable. Range: 1 to 65535
Pin
This variable contains authorization PIN for telephone procedures. 'none' = inactive (can not be dialed). Length: 4 to 4
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)
Facilities
user facilities. userBusyOnBusy: if set, all incoming calls for this user are rejected with user busy, if at least one number of this user is busy. Enumerations: userBusyOnBusy (0)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH