>> MIB - Management Information Base
>> Table: pimBidirDFElectionTable - (.1.3.6.1.4.1.272.4.5.54.2.1.10.1)
Description: An entry (conceptual row) in the pimBidirDFElectionTable.
pimBidirDFElectionTable
OID | Name | Type | Access
.1 | AddressType | ENUM | R
.2 | RPAddress | InetAddressIPv6 | R
.3 | IfIndex | InterfaceIndex | R
.4 | WinnerAddressType | ENUM | R
.5 | WinnerAddress | InetAddressIPv6 | R
.6 | WinnerUpTime | TimeTicks | R
.7 | WinnerMetricPref | Unsigned32 | R
.8 | WinnerMetric | Unsigned32 | R
.9 | State | ENUM | R
.10 | StateTimer | TimeTicks | R
AddressType
The address type of the RP for which the DF state is being maintained. Enumerations: unknown (0) ipv4 (1) ipv6 (2) ipv4z (3) ipv6z (4) dns (16)
RPAddress
The IP address of the RP for which the DF state is being maintained. The InetAddressType is given by the pimBidirDFElectionAddressType object. Length: 16 to 16
IfIndex
The value of ifIndex for the interface for which the DF state is being maintained. Range: 1 to 2147483647
WinnerAddressType
The primary address type of the winner of the DF Election process. A value of unknown(0) indicates there is currently no DF. Enumerations: unknown (0) ipv4 (1) ipv6 (2) ipv4z (3) ipv6z (4) dns (16)
WinnerAddress
The primary IP address of the winner of the DF Election process. The InetAddressType is given by the pimBidirDFElectionWinnderAddressType object. Length: 16 to 16
WinnerUpTime
The time since the current winner (last) became elected as the DF for this RP.
WinnerMetricPref
The metric preference advertised by the DF Winner, or zero if there is currently no DF.
WinnerMetric
The metric advertised by the DF Winner, or zero if there is currently no DF.
State
The state of this interface with respect to DF-Election for this RP. The states correspond to the ones defined in the BIDIR-PIM specification. Enumerations: dfOffer (1) dfLose (2) dfWinner (3) dfBackoff (4)
StateTimer
The minimum time remaining after which the local router will expire the current DF state represented by pimBidirDFElectionState.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH