>> MIB - Management Information Base
>> Table: wlcACAddressTable - (.1.3.6.1.4.1.272.4.61.1.2.1)
Description: This table lists the IP address type and the IP address of the AC
wlcACAddressTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | InetType | ENUM | RW
.3 | InetAddress | IpAddress | RW
.4 | AdminStatus | ENUM | D
Index
Unique index of an accessible AC.
InetType
IP address type. Possible values are: -unknown(0): an unknown address type -ipv4(1) : an IPv4 address -ipv6(2) : an IPv6 address -ipv4z(3) : a non-global IPv4 address including a zone index -ipv6z(4) : a non-global IPv6 address including a zone index -dns(16) : a DNS domain name Enumerations: unknown (0) ipv4 (1) ipv6 (2) ipv4z (3) ipv6z (4) dns (16)
InetAddress
The IP address of the accessbile AC.
AdminStatus
Enable, disable or delete the requested AC address. Enumerations: disabled (1) enabled (2) delete (32)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH