>> MIB - Management Information Base
>> Table: wlcWTPStatTable - (.1.3.6.1.4.1.272.4.61.1.43.1)
Description: Contains additional WTP statistics
wlcWTPStatTable
OID | Name | Type | Access
.1 | WTPIndex | INTEGER | R
.2 | Temperature | INTEGER | R
.3 | CPU | INTEGER | R
.4 | FreeMemory | Unsigned32 | R
.5 | TotalMemory | Unsigned32 | R
.6 | PortLinkStatus | ENUM | R
WTPIndex
Index of the WTP
Temperature
Numeric value of the main sensor of the WTP in Celsius.
CPU
Numeric value of the main CPU usage in percentage. Range: 0 to 100
FreeMemory
Free dram available in bytes.
TotalMemory
Total dram available in bytes.
PortLinkStatus
Speed of the WTP link used for communicating with the WLC Enumerations: down (1) half-10 (2) full-10 (3) half-100 (4) full-100 (5) half-1000 (6) full-1000 (7) half-2500 (8) full-2500 (9)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH