>> MIB - Management Information Base
>> Table: xauthProfileTable - (.1.3.6.1.4.1.272.4.26.18.1)
Description: This object contains an XAUTH profile.
xauthProfileTable
OID | Name | Type | Access
.1 | Index | Unsigned32 | RW
.2 | Description | DisplayString | RW
.3 | Role | ENUM | RW
.4 | Mode | ENUM | RW
.5 | AAAServerGroupId | INTEGER | RW
.6 | UserListGroupId | INTEGER | RW
.7 | Timeout | INTEGER | RW
.8 | AdminStatus | ENUM | D
Index
A unique index identifying this entry.
Description
An optional description for this profile, only used for descriptive purposes (max. 50 characters).
Role
This object specifies which role is choosed for this profile. Possible values: server(1) -- XAUTH is used and local device is the XAUTH server, i.e. this side requests extended authentication client(2) -- XAUTH is used and local device is the XAUTH client, i.e. this side responds with its extended authentication credentials
Mode
This object specifies the kind how to get user data for authentication. Possible values: local(1), -- user data are configured locally in the entries of xauthUserListTable that are referenced by xauthPrfUserListGroupId radius(1) -- user data are configured at RADIUS server, RADIUS server is referenced by xauthPrfAAAServerGroupId that corresponds to radiusSrvGroupId in radiusSrvTable, 'radius' mode is only valid for server role
AAAServerGroupId
This object specifies the group ID which is used for RADIUS authentication to find the associated server entry in radiusSrvTable for XAUTH. See description of radiusSrvGroupId for details. This object is only valid for entries with xauthPrfMode 'radius'.
UserListGroupId
This object refers to a group of one or more user entries in xauthUserListTable. This object is only valid for entries with xauthPrfUserMode 'local'.
Timeout
WARNING: this object is obsolete and must not be used.
AdminStatus
MIB entry deletion is performed by this object: - enable : enables xauthPrfTable entry - delete : deletes xauthPrfTable entry.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH